**Building Inspections** required for occupancy:

1. Egress requirements
2. Fire extinguisher placement
3. Railing and stair requirements complete
4. Fire and smoke stopping complete
5. Fire rated assemblies in place
6. Accessibility code requirements are satisfied
7. Safe access to site
8. Insure that all trade finals are complete
9. Signage complete
10. Architecturally complete
11. Site engineering components complete
12. Site landscaping components complete

**Mechanical Inspections** required for occupancy:

1. Smoke damper inspection.

2. Fire damper inspection.

3. Test and balance report including differential pressure readings for smoke detectors.

4. Controls inspection.

5. Hood test including velocity requirements (T+B of system).

6. Flammable storage alarm test.

**Plumbing Inspections** required for occupancy:

1. Drainage completion

2. Sewer connection.

3. Water system completion.

4. Interior plumbing systems

**Electrical Inspections** required for occupancy:

1. Hot check for complete electrical system.
2. Completion of emergency lighting system.
3. Completion of lightning protection system.

4. Completion of intercom system

5. Generator Testing

**Fire Inspections** required for occupancy:

1. Fire alarm
2. Fire sprinkler system
3. Kitchen hood
4. Fire sprinkler pump